DATE: NAME:

|  |  |
| --- | --- |
| **Equipment ID’s** |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **ALL ITEMS** | **Acceptable** | **Not Acceptable** | **N/A** |
| Identification |  |  |  |
| Lifespan |  |  |  |
| Manufacturer’s instructions |  |  |  |
| Previous Inspection/Use records |  |  |  |
| Realistic Operational check |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **METAL ITEMS/ COMPONENTS** | **Acceptable** | **Not Acceptable** | **N/A** |
| Build-up of foreign matter |  |  |  |
| Burring |  |  |  |
| Contamination by chemicals |  |  |  |
| Corrosion |  |  |  |
| Cracks |  |  |  |
| Cuts |  |  |  |
| Deformation / buckling |  |  |  |
| Heavy marking or scoring |  |  |  |
| Moving parts function correctly |  |  |  |
| Pivot action and component wear |  |  |  |
| Wear |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **HELMETS** | **Acceptable** | **Not Acceptable** | **N/A** |
| Contamination to cradle & straps |  |  |  |
| Contamination to shell |  |  |  |
| Cracks/Cuts in shell |  |  |  |
| Damage to cradle and straps |  |  |  |
| Deformation of shell |  |  |  |
| Heavy marking or scoring |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **TEXTILE ITEMS/COMPONENTS** | **Acceptable** | **Not Acceptable** | **N/A** |
| Concealed Surfaces - Abrasion |  |  |  |
| Cuts |  |  |  |
| Damage by chemicals |  |  |  |
| Damage by heat, glazed areas |  |  |  |
| Dirty |  |  |  |
| Discolouration |  |  |  |
| Fittings, fastening & buckles |  |  |  |
| General Surfaces - Abrasion |  |  |  |
| Hardened areas |  |  |  |
| Internal damage |  |  |  |
| Knots |  |  |  |
| Knots tightness |  |  |  |
| Length of end tails of knots |  |  |  |
| Powdery surface |  |  |  |
| Stitching: cut, broken or abraded |  |  |  |

|  |
| --- |
| **Candidates Recommendations:**  🞏 Remove Item from Service 🞏 Item Fit for Continued Use |